Report

|  |
| --- |
|  |

|  |  |
| --- | --- |
| Prepared by: | Prepared for: |
|  |  |
| SDC Verifier |  |
|  |  |

|  |  |
| --- | --- |
| Engineer: |  |
| Customer: |  |
| Project Number: |  |
| Version: | 1 |
| Date: | 1 Sep 2014 |

# Preface

This document is generated with SDC Verifier 3.6.1 and calculated with FEMAP v11.1.0

Model File: D:\SDC\AISC Examples\Chapter E\Example E1B-1D\Example\_E.1B\_and\_E.1D\_v11\_1.modfem

Project File: D:\SDC\AISC Examples\Chapter E\Example E1B-1D\Example\_E.1B\_and\_E.1D\_v11.sdcv

Report Profile: 1..Standards

For further questions on the program contact us:

tel: +31 15 30 10 310  
email: support@sdcverifier.com  
Zijlvest 25  
2011VB Haarlem  
Netherlands

Femap and SDC Verifier models coincide. Checked information is presented below:

|  |  |  |
| --- | --- | --- |
| Entity | Femap Model Entities Count | SDC Verifier Model Entities Count |
| Nodes | 11 | 11 |
| Elements | 10 | 10 |
| Materials | 1 | 1 |
| Property | 1 | 1 |

# Model Entities

This paragraph shows detailed or brief model overview.

## Materials

This paragraph contains materials information.

### Materials Summary

|  |  |  |  |
| --- | --- | --- | --- |
| Title | Element(s) | Mass | Gravity Center |
| 1..Steel ASTM A992 | 10 | 4674600.00 | [180.00; 0.00; 0.00] |

### 1..Steel ASTM A992

|  |  |
| --- | --- |
| Property | Value |
| Elements | 10 |
| Mass | 4674600.00 |
| Gravity Center | [180.00; 0.00; 0.00] |
| X [Min;Max] | [0.00; 360.00] |
| Y [Min;Max] | [0.00; 0.00] |
| Z [Min;Max] | [0.00; 0.00] |

|  |  |  |
| --- | --- | --- |
|  | Property | Value |
| FEM Relevant | Young Modulus | 2.90e+07 |
|  | Shear Modulus | 0.00 |
|  | Poisson Ratio | 0.30 |
|  | Shear | 0.00 |
|  | Mass Density | 490.00 |
| SDC Verifier Relevant | Tensile Strength | 0.07e+6 |
|  | Yield Stress | 0.05e+6 |
|  | | | |

## Properties

This paragraph contains properties information.

### Properties Summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Title | Element(s) | Material | Mass | Gravity Center |
| 1..W14x90 | 10 | 1..Steel ASTM A992 | 4674600.00 | [180.00; 0.00; 0.00] |

### 1..W14x90

|  |  |
| --- | --- |
| Property | Value |
| Elements | 10 |
| Type | Beam |
| Material | 1..Steel ASTM A992 |
| Mass | 4674600.00 |
| Gravity Center | [180.00; 0.00; 0.00] |
| X [Min;Max] | [0.00; 360.00] |
| Y [Min;Max] | [0.00; 0.00] |
| Z [Min;Max] | [0.00; 0.00] |
| Moment I1 or Izz | 999.00 |
| Moment I2 or Iyy | 362.00 |
| Moment I3 or Izy | 0.00 |
| Area A | 26.50 |
| Z Shear Area | 17.78 |
| Y Shear Area | 5.50 |
| Torsional Constant J | 4.06 |
| Nonstructural Mass Length | 0.00 |
| Warping Constant | 16000.00 |
| Perimeter | 85.12 |
| Y Neutral Axis Offset | 0.00 |
| Z Neutral Axis Offset | 0.00 |

|  |  |
| --- | --- |
|  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Geometry Property | Value | Points Of Interest | Value |
| Height | 14.00 | Point 1 | [-7.00 ; 7.25] |
| Width | 14.50 | Point 2 | [-7.00 ; -7.25] |
| h | 14.00 | Point 3 | [7.00 ; -7.25] |
| a | 14.50 | Point 4 | [7.00 ; 7.25] |
| b | 14.50 |  |  |
| c | 0.71 |  |  |
| d | 0.44 |  |  |
| t | 0.71 |  |  |
|  | | | | |

## FEM Loads

This paragraph contains information about applied loads to model.

### 1..Dead load (140 kips)

|  |  |  |  |
| --- | --- | --- | --- |
| Definition Title | Load Type | Applied on | Value(s) |
| 1..Force on Node | Force | Node: 11 | (-140000;0;0) |

|  |
| --- |
|  |

### 2..Live load (420 kips)

|  |  |  |  |
| --- | --- | --- | --- |
| Definition Title | Load Type | Applied on | Value(s) |
| 1..Force on Node | Force | Node: 11 | (-420000;0;0) |

|  |
| --- |
|  |

## Constraints

This paragraph contains information about constrained parts of the model.

### 1..Pinned

|  |  |  |
| --- | --- | --- |
| Definition | Count | Type (DOF) |
| 1..Top | 1 node(s) | Ty Tz Rx |
| 2..Bottom | 1 node(s) | Tx Ty Tz Rx |
| 3..Ty;Rx | 1 node(s) | Ty Rx |
|  | | | |

# Standards

This paragraph shows detailed information about applied standards.

## 1..ANSI / AISC LRFD 360-10

#### General Information

|  |  |
| --- | --- |
| Property | Value |
| Title | ANSI / AISC LRFD 360-10 |
| Type | 11 |
| Constants | 8 |
| Classifications | 0 |
| Standard Tables | 0 |

### Constant

|  |  |
| --- | --- |
| Title | Value |
| F\_t | 0.9 |
| F\_c | 0.9 |
| F\_v | 0.9 |
| rolled | 1 |
| built\_up | 2 |
| nonslender | 3 |
| slender | 4 |
| NotSupported | -12345678 |

### Characteristics

This paragraph contains information about extra elemental characteristics

#### 1..Section Build Type

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Section\_Build\_Type |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | 1..W14x90 | 1 |  |  |  |

|  |
| --- |
|  |

#### 1..Beam Length Y

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Ly |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | Beam Member 1 | 360 |  |  |  |

|  |
| --- |
|  |

#### 2..Effective Length Factor Y

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Ky |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | Beam Member 1 | 1 |  |  |  |

|  |
| --- |
|  |

#### 3..Beam Length Z

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Lz |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | Beam Member 1 | 180 |  |  |  |

|  |
| --- |
|  |

#### 4..Effective Length Factor Z

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Kz |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | Beam Member 1 | 1 |  |  |  |

|  |
| --- |
|  |

#### 5..Torsional Length

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Ltor |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | All Entities | 180 |  |  |  |

|  |
| --- |
|  |

#### 6..Effective Torsional Length

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | Ktor |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | All Entities | 1 |  |  |  |

|  |
| --- |
|  |

#### 7..Stiffener Distance

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | a |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | All Entities | 0 |  |  |  |

|  |
| --- |
|  |

#### 8..Net Area

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | An |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | All Entities | 0 |  |  |  |

|  |
| --- |
|  |

#### 9..Shear Lag Factor

|  |  |
| --- | --- |
| Property | Value |
| Type |  |
| AliasName | U |
| Groups count | 1 |

#### Description

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Property | Value | No. | Property | Value |
| 1 | AllEntities | 0 |  |  |  |

|  |
| --- |
|  |

### Checks

This paragraph contains checks descriptions with their results.

#### 1..Beam Characteristics

|  |  |
| --- | --- |
| Property | Value |
| Category | Elemental Custom Check |
| Selection | 18 PropertyShape(s) |
| Parameters | 8 |

All (LS1, All Entities)

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Check | | 1..Beam Characteristics | | | | Load Set: | | 1..LRFD | | | |
| Selection | | All Entities | | | | Direction | | All | | | |
| Load | Radius of Gyration Y | | Radius of Gyration Z | Slenderness Ratio Y | Slenderness Ratio Z | | Elastic Buckling Stress Y | | Elastic Buckling Stress Z | Critical Stress Y Q1 | Critical Stress Z Q1 | |
| Load Set '1..LRFD' | 6.14 | | 3.70 | 58.63 | 48.70 | | 83255.38 | | 120674.48 | 38886.91 | 42039.17 | |

#### 9..Axial

|  |  |
| --- | --- |
| Property | Value |
| Category | Elemental Custom Check |
| Selection | 17 PropertyShape(s) |
| Parameters | 4 |

All (LS1, All Entities)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Check | 9..Axial | | | Load Set: | | 1..LRFD | |
| Selection | All Entities | | | Direction | | All | |
| Load | | Nominal Compressive Strength | Design Tensile Strength | | Axial Force | | Utilization Factor | |
| Load Set '1..LRFD' | | 927452.81 | 1192500.00 | | -840000.00 | | 0.91 | |